# SSHCZO Metadata Worksheet

|  |  |
| --- | --- |
| Data File Name | **CF\_CFW\_W2.csv** |
| Date Prepared | 2018-07-18 |
| Descriptive Title | CFW\_2: Cole Farm Well 2 |
| Update Frequency | Quarterly |
| Abstract | Groundwater level data and water temperature for CFW\_2 measured every 15 minutes using a HOBO U20-001-01 non-vented pressure transducer from 2018-02-23 to present. Sensor level during this period is set to 9.59 meters below ground level. |
| Investigator  Contact Info | Dr. Susan Brantley, Professor of Geosciences, The Pennsylvania State University, 2217 Earth and Environmental Systems Institute, University Park, PA, 16802, 814.865.1619, [sxb7@psu.edu](mailto:sxb7@psu.edu). |
| Data Value Descriptions | * COL1: label = TmStamp\_UTC; Timezone = Coordinated Universal Time * COL2: label = WaterTemp\_C; water temperature; Units = degC * COL3: label = Abs\_Press\_Barom\_kPa; barometric pressure; Units = kPa * COL4: label = WL\_BLG\_m; water level below ground; Units = meters |
| Keywords | Groundwater Depth, Groundwater Temperatures, Hydrology |
| Methods | Groundwater level measurements are recorded every 15 minutes on a HOBO U20-001-01 non-vented pressure transducer. Data are manually downloaded monthly using HOBO-Ware Pro software. Sensor depth is calculated in the software by processing with barometric pressure data recorded on a separate HOBO U20-001-01 pressure transducer. Water level below ground determined using the suspended cable length to sensor below ground and taking the difference of the SensorDepth\_m [WL\_BLG\_m = 9.59 - SensorDepth\_m].  TOC above land surface = 0.3 meters  Sensor location down borehole from MP = 9.89 meters  Well Depth = 37.795 meters  Casing type = steel  Casing diameter = 15.2 cm  Casing depth = 6.401 meters  The water table below land surface obtained by subtracting the head pressure and above ground casing length from the sensor depth.  Quality control:  Data were checked by graphing data in R package and comparing to precipitation and manual water level measurements using a Solinist electric tape. Bad, missing, or erroneous data values were removed or marked with -9999 which could be caused during data downloads and/or malfunctioning sensors.  Data gaps present:  2018-04-17: sensor removed during well sampling  Explained data variations:  2018-07-11: well was pumped/sampled with sensor in place from 14:00 to 15:30 |
| Sites | Cole Farm, Huntingdon County, Barree Township Lat/Long DMS: 40.636272/ -77.938443; (NAD\_1983\_StatePlane\_Pennsylvania\_South\_FIPS\_3702); Elevation 269.138m |
| Publications | none |
| Citation | The following acknowledgment should accompany any publication or citation of these data: Logistical support and/or data were provided by the NSF-supported Susquehanna Shale Hills Critical Zone Observatory. |
| Data Use Notes | The user of Susquehanna Shale Hills CZO data agrees to provide proper acknowledgment with each usage of the data. Citation of the name(s) of the investigator(s) responsible for the data set, in addition to the generic statement above, constitutes proper acknowledgment. Author(s) (including Susquehanna Shale Hills CZO investigators) of published material that makes use of previously unpublished Susquehanna Shale Hills CZO data agree to provide the Susquehanna Shale Hills CZO data manager with four (4) copies (preferably reprints) of that material for binding as soon as it becomes available. The user of Susquehanna Shale Hills CZO data agrees not to resell or redistribute shared data. The user of these data should be aware that, while efforts have been taken to ensure that these data are of the highest quality, there is no guarantee of perfection for the data contained herein and the possibility of errors exists. These data are defined as either public or private, such that a password may be required for access. |