# CZO Metadata Worksheet

|  |  |
| --- | --- |
| Data File Name | Soil Gas Concentration Data |
| Date Prepared | 4/10/2014 |
| Descriptive Title | Shale Hills CZO Soil Gas Concentration and Flux Data (Level 0) |
| Update Frequency | Monthly (sporadic) |
| Abstract | The soil CO2 and N2O concentrations and various soil properties for the planar slope and swale sampling locations in the Susquehanna Shale Hills Critical Zone Observatory watershed. |
| Investigator  Contact Info | Dr. Elizabeth Hasenmueller, Postdoctoral Scholar, The Pennsylvania State University, 116 ASI Building, University Park, PA 16801, 1-814-863-5905, [eah262@psu.edu](https://sn2prd0202.outlook.com/owa/redir.aspx?C=wuhkEuXJKkugLW0Us0un5wlW9x5-wM8I7us7kKL25Pg3NFvEgUrl1_u8dYMW2Ma-iTJaJogVdmg.&URL=mailto%3aeah262%40psu.edu).  Julie Weitzman, Graduate Student, The Pennsylvania State University, 116 ASI Building, University Park, PA 16801, 1-814-863-9804, [jnw142@psu.edu](mailto:jnw142@psu.edu). |
| Data Value Descriptions | 2008 – 2010:   * COL1: label=Sample Label. * COL2: label=Sample Location. * COL3: label=Local time of day, Time Zone=EST. * COL4: label=Date. * COL5: label=Julian day. * COL6: label=Soil depth (m). * COL7: label=Order # (for injection of samples into the LICOR 7000 for analysis). * COL8: label=CO2 concentration (ppm). * COL9: label=Soil porosity. * COL10: label= Soil VWC (m3/m3). * COL11: label=Air Temperature (°C). * COL12: label=Soil Temperature (°C). * COL13: label=Elevation (m).   2013:   * COL1: label=Site Name * COL2: label=Date * COL3: label=Depth (cm) * COL4: label=CO2 concentration (ppm) * COL5: label= N2O concentration (ppm) |
| Keywords | CO2 Concentration, Soil CO2, N2O Concentration, Soil N2O, CO2 Flux |
| Methods | 2008 – 2010:   * CO2 concentration data were measured using a LICORE 7000. * Soil VWC was measured with a time domain reflectometer. * Air temperatures were obtained from the RTHnet website. * Soil temperature were measured using a ST09 Supco soil temperature probe * Gas sampler elevations were measured using a Garmin GPSmap 76CSx GPS.   2013:   * Soil gas measured in situ using a Model 1412 Infrared Photoacoustic Spectroscopy (PAS) gas analyzer powered by a model EU1000i portable electric Honda generator. All gas flux sampling took place between 09:00 and 13:00 hours – the time of lowest diurnal temperature variability. |
| Citation | The following acknowledgment should accompany any publication or citation of these data: Logistical support and/or data were provided by the NSF-supported Shale Hills Susquehanna Critical Zone Observatory. |
| Publications | None |
| Data Use Notes | The user of Shale Hills Susquehanna CZO data agrees to provide proper acknowledgment with each usage of the data. Citation of the name(s) of the investigator(s) responsible for the data set, in addition to the generic statement above, constitutes proper acknowledgment. Author(s) (including Shale Hills Susquehanna CZO investigators) of published material that makes use of previously unpublished Shale Hills Susquehanna CZO data agree to provide the Shale Hills Susquehanna CZO data manager with four (4) copies (preferably reprints) of that material for binding as soon as it becomes available. The user of Shale Hills Susquehanna CZO data agrees not to resell or redistribute shared data. The user of these data should be aware that, while efforts have been taken to ensure that these data are of the highest quality, there is no guarantee of perfection for the data contained herein and the possibility of errors exists. These data are defined as either public or private, such that a password may be required for access. |