# SSHCZO Metadata Worksheet

|  |  |
| --- | --- |
| Data File Name | **SSHCZO\_CFEMS\_airtemp\_RH\_Precip\_Level\_0.csv** |
| Date Prepared | 2018-05-23 |
| Descriptive Title | Air Temperature, Relative Humidity, and Precip |
| Update Frequency | Monthly |
| Abstract | Raw (not quality controlled) precipitation, air temperature, and relative humidity are measured and recorded meteorological instruments on the Cole Farm East Mid-Slope station at the Cole Farm property. Data are manually downloaded monthly and imported to the SSHCZO database.  |
| InvestigatorContact Info | Dr. Li Li, Associate Professor, Department of Energy and Mineral Engineering, The Pennsylvania State University, 154 Hosler Building, University Park, PA 16802, (814)867-3547 lili@eme.psu.eduDacheng Xiao, PhD student, Department of Energy and Mineral Engineering, The Pennsylvania State University, 228 Hosler Building, University Park, PA 16802, (814)777-6006dzx102@psu.edu |
| Data Value Descriptions | * COL1: label = TmStamp, TimeZone=UTC.
* COL2: label = Record, data logger sequential system
* COL3: label = AirTC\_Avg, TimeSupport= 10 min, Units = Degrees C
* COL4: label = RelativeHumidity, TimeSupport= 10 min, Units %
* COL5: label = Rain\_mm\_Tot, TimeSupport= 10 min, Units = mm
 |
| Keywords | Air temperature, relative humidity, precipitation, rain |
| Methods | Air temperature and relative humidity are measured every 10 minutes using a Campbell Scientific CS215 sensor. Air temperature and relative humidity are measured every 30 seconds over the 10 minute period with the final value being averaged and recorded. Preciptitation (rain) is measured every 10 minutes with a Texas Electronics tipping bucket rain gauge. Both sensors are mounted on 1.5 meter tripod wired to a Campbell Scientific CR1000 data logger.  |
| Sites | Sites:* Cole Farm:

|  |  |
| --- | --- |
| Name | Cole Farm East Mid-Slope |
| Latitude | 40.636397 |
| Longitude | -77.942061 |

 |
| Publications | none |
| Citation | The following acknowledgment should accompany any publication or citation of these data: Financial Support was provided by National Science Foundation Grant EAR – 1331726 (S. Brantley) for the Susquehanna Shale Hills Critical Zone Observatory.  Logistical support and/or data were provided by the NSF-supported Susquehanna Shale Hills Critical Zone Observatory.Acknowledgement for research in Cole Farm:This research was conducted on a farm in Shaver's Creek watershed at the intersection of RT 305 and Winchester Road. |
| Data Use Notes | The user of Susquehanna Shale Hills CZO data agrees to provide proper acknowledgment with each usage of the data. Citation of the name(s) of the investigator(s) responsible for the data set, in addition to the generic statement above, constitutes proper acknowledgment. Author(s) (including Susquehanna Shale Hills CZO investigators) of published material that makes use of previously unpublished Susquehanna Shale Hills CZO data agree to provide the Susquehanna Shale Hills CZO data manager with four (4) copies (preferably reprints) of that material for binding as soon as it becomes available. The user of Susquehanna Shale Hills CZO data agrees not to resell or redistribute shared data. The user of these data should be aware that, while efforts have been taken to ensure that these data are of the highest quality, there is no guarantee of perfection for the data contained herein and the possibility of errors exists. These data are defined as either public or private, such that a password may be required for access. |